{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["2_ДОПОГ"]
["№ п/п","Вопрос","Варианты ответа",null,"Обоснование"]
[1,"Разрешено ли водителю, перевозящему опасные грузы, прошедшему базовый курс подготовки согласно ДОПОГ, осуществлять перевозку газов в баллонах?","Не разрешено","правильно","ДОПОГ п. 8.2.1.1"]
[null,null,"Разрешено "]
[null,null,"Разрешено, если максимальная разрешенная масса транспортного средства не превышает 3,5 т."]
[2,"Общая вместимость топливных баков на одну транспортную единицу, перевозящую опасные грузы, не должна превышать :",1500,"правильно","ДОПОГ п. 1.1.3.3"]
[null,null,"1000 литров"]
[null,null,"500 литров"]
[null,null,"Количество литров не ограничено."]